Note that the NRF in lab uses SDK 15.3.0

Reference: SPIM SDK 15.3.0 Driver

<https://infocenter.nordicsemi.com/topic/com.nordic.infocenter.sdk5.v15.3.0/group__nrfx__spim.html>

~/eecs149-proj/nRF5\_SDK\_15.3.0\_59ac345/examples/peripheral/spi/pca10056/blank/config is where pins are defined e.g. SPI\_SS\_PIN, SPI\_MISO\_PIN